UoMaine underway optics Eventlog

## Leg 8 Salvador – Rio

T.linkowski

17/10/2021

**11:40 UTC**, System started once in open water.

23/10/2021

**12:00 UTC**, system stopped. Optics on ACS, HBB and Seapoint cleaned. Coarse filters cleaned. Tubing cleaned.

**21:05 UTC**, system restarted

29/10/2021

**20:30 UTC**, Pump stopped Optics on ACS, HBB and Seapoint cleaned. Filters checked and no sign of dirt or particles.

**23:20 UTC**, System restarted

30/10/2021

**21:00 UTC**, Pump stopped, coarse filter cleaned because full of crabs larvaes. Pre-filter changed. Tubing and chamber on ACS leaking, silicone applied around lenses, Stainless hose clamp installed to reduce leakage.

**22:00 UTC**, system restarted

02/11/2021

**19:30 UTC**, System stopped to clean optics on ACS, HBB and Seapoint. ACS leakage less important but still has drops where tubing are attached to the chamber.

**23:15 UTC**, System restarted.